Overview | Project | Class | Tree | Deprecated | Index

Nestopia Core API

FRAMES NO FRAMES
SUMMARY: INNER | FIELD | CONSTR | METHOD

## api
Class Nes::Api::Fds

    Base
       |
       +--Nes::Api::Fds

class Nes::Api::Fds
extends Base

Famicom Disk System interface.

Inner Classes, Typedefs, and Enums
`typedef` | `Nes::Api::Fds::DiskCallback` Disk event callback prototype.
`struct` | `Nes::Api::Fds::DiskData` Disk data context.
`typedef` | `Nes::Api::Fds::DriveCallback` Drive event callback prototype.
`enum` | `Nes::Api::Fds::Event` Disk event.
`enum` | `Nes::Api::Fds::Motor` Drive event.

Field Summary
`static Nes::Api::Fds::DiskCaller` | `diskCallback` Disk event callback manager.
`static Nes::Api::Fds::DriveCaller` | `driveCallback` Drive event callback manager.

Constructor Summary
`Fds( T& instance )` Interface constructor.

Method Summary
`bool` | `CanChangeDiskSide() const` Checks if the current disk can change side.
`Result` | `ChangeSide()` Changes disk side.
`Result` | `EjectDisk()` Ejects disk.
`Result` | `GetBIOS( std::ostream& stream ) const` Stores the current BIOS in an output stream.
`int` | `GetCurrentDisk() const` Returns the current disk inserted.
`int` | `GetCurrentDiskSide() const` Returns the current disk side.
`Result` | `GetDiskData( uint side, Nes::Api::Fds::DiskData& data ) const` Returns disk information.
`uint` | `GetNumDisks() const` Returns the total number of disks.
`uint` | `GetNumSides() const` Returns the total number of disks and their sides.
`bool` | `HasBIOS() const` Checks if a BIOS has been loaded.
`bool` | `HasHeader() const` Checks if the current loaded image comes with a file header.
`Result` | `InsertDisk( uint disk, uint side )` Inserts a disk.
`bool` | `IsAnyDiskInserted() const` Checks if a disk is inserted.
`Result` | `SetBIOS( std::istream* stream )` Sets BIOS.

Field Detail

### diskCallback

    public static Nes::Api::Fds::DiskCaller diskCallback;

  Disk event callback manager. Static object used for adding the user defined callback.

### driveCallback

    public static Nes::Api::Fds::DriveCaller driveCallback;

  Drive event callback manager. Static object used for adding the user defined callback.

Constructor Detail

### Fds

    public Fds( T& instance );

  Interface constructor.

Parameters:
  `instance` - emulator instance

Method Detail

### CanChangeDiskSide

    public bool CanChangeDiskSide() const throw();

  Checks if the current disk can change side.

Returns:
  true if disk can change side

### ChangeSide

    public Result ChangeSide() throw();

  Changes disk side.

Returns:
  result code

### EjectDisk

    public Result EjectDisk() throw();

  Ejects disk.

Returns:
  result code

### GetBIOS

    public Result GetBIOS( std::ostream& stream ) const throw();

  Stores the current BIOS in an output stream.

Parameters:
  `output` - stream
Returns:
  result code

### GetCurrentDisk

    public int GetCurrentDisk() const throw();

  Returns the current disk inserted.

Returns:
  current disk or NO_DISK if none

### GetCurrentDiskSide

    public int GetCurrentDiskSide() const throw();

  Returns the current disk side.

Returns:
  0(A), 1(B) or NO_DISK if no disk inserted

### GetDiskData

    public Result GetDiskData( uint side, Nes::Api::Fds::DiskData& data ) const throw();

  Returns disk information.

Parameters:
  `side` - disks and sides index
  `data` - object to be filled
Returns:
  result code

### GetNumDisks

    public uint GetNumDisks() const throw();

  Returns the total number of disks.

Returns:
  number

### GetNumSides

    public uint GetNumSides() const throw();

  Returns the total number of disks and their sides.

Returns:
  number

### HasBIOS

    public bool HasBIOS() const throw();

  Checks if a BIOS has been loaded.

Returns:
  true if a BIOS has been loaded.

### HasHeader

    public bool HasHeader() const throw();

  Checks if the current loaded image comes with a file header.

Returns:
  true if it comes with a file header

### InsertDisk

    public Result InsertDisk( uint disk, uint side ) throw();

  Inserts a disk.

Parameters:
  `disk` - disk number
  `side` - disk side, 0(A) or 1(B)
Returns:
  result code

### IsAnyDiskInserted

    public bool IsAnyDiskInserted() const throw();

  Checks if a disk is inserted.

Returns:
  true if a disk is inserted

### SetBIOS

    public Result SetBIOS( std::istream* stream ) throw();

  Sets BIOS.

Parameters:
  `input` - stream to ROM binary or iNES file, set to NULL to remove current BIOS

Overview | Project | Class | Tree | Deprecated | Index

Nestopia Core API

FRAMES NO FRAMES
SUMMARY: INNER | FIELD | CONSTR | METHOD